888 Longfellow Addendum

* Garage footprint will remain the same with the same front door and access door dimensions and placement.
* Garage roof will remain with the same shingles but roofline will be of a standard gable design with an 8/12 pitch (see attachment below)
* Garage roof overhang of 1’
* Garage Wall

Garage wall info Wall Info:  
Siding Material Types: Fiber Cement Siding  
Siding: AlluraTM 5/16" x 7-1/4" x 12' Smooth Fiber Cement Lap Siding Siding Color: Primed  
Accent Material Type: None  
Wainscot Material Type: None  
House Wrap: Kimberly-Clark BLOCK-IT®9'x75'House Wrap  
Gable Vents: Novik® 16" Octagon Gable Vent  
Gable Vent Color: ABT Co - White - 001  
Walls Sheathing: 7/16" OSB (Oriented Strand Board)

* All garage trim, fascia and soffit of smooth cement fiberboard
* Garage cladding will be 12’ reveal smooth lap cement board or with a reveal acceptable to the DHC. Painted to match existing home.

