Window Renovation – East Elevation (one photo):

1,2 – basement, full size sash window pair. Found buried and intact. Removed, stripped, repaired and placed back into original openings.

3,6 – found in garage, stripped, repaired, reglazed. Replaced vinyl windows that was broken. Old replacement removed along with all breakmetal surrounding. Trim on outside cleaned and painted, inside frame from original installation still intact. Replaced brass insulating strips with identical new. Reglazed and stripped old window left in attic and rebuilt and reinstalled.

4,5 – replaced Vinyl window with windows from attic. Windows are wood framed and 6 individual pains of glass. These were original windows from the attic. Same process as previously explained. Windows are operable.

8-12 – All are double hung, sash windows. All are original windows that were removed from their frames, stripped and reglazed. All working hardware was reconditioned. Only new materials used in any of the rebuilds is the rope for the counterweights. All tracks were restored. No new glass was used.

13 – attic window will not be replaced

7 – Original window is currently being disassembled and reconditioned. No work is being done now.

\*\*\*\*\*\*Note\*\*\*\* In removing the vinyl replacement windows, and break metal surrounding the windows, it was remarkably discovered that the frames are in perfect condition as built originally. All the original windows are in near perfect condition once paint and glazing is removed.

\*\*NOTE\*\* Only original windows are being used. These are all wood construction, some double hung and some fixed, and some operable as indicated. If approved where original windows are not found, I would like to custom construct the window with the configuration it was originally made to using hardwoods and period hardware to match the rest of the house.