Window Renovation – South Elevation (3 photos):

14 – Vinyl windows to be replaced with found windows from attic which are wood framed and the exact configuration as vinyl. The windows are double hung sash windows that are being reinstalled. The condition of the old windows is excellent. Same window configuration as show in the vinyl window. Same process of stripping and repairing.

15 – Original windows that were still installed in opening. Windows were removed and cleaned, repaired and reglazed.

16 – windows found in attic and are being restored as previously described. These windows are a combination of operable (one swings from left and one from right on brass hinges). Left to right are fixed, operable, fixed, operable, fixed. Hinge locations still on frames indicating the original configuration.

17- original window restored.

18 – 22 – currently showing the vinyl windows. Original windows to be installed after restoration.

23 – attic window vinyl, not found in pile of old windows. I would like to have this window custom made to match the original windows in the house.

\*\*NOTE\*\* Only original windows are being used. These are all wood construction, some double hung and some fixed, and some operable as indicated. If approved where original windows are not found, I would like to custom construct the window with the configuration it was originally made to using hardwoods and period hardware to match the rest of the house.