**1080 IROQUOIS –** *italics indicate operational change*

**Front:**

Three openings -

Triple slider to be replaced with gliding windows to match current sash dimensions

*Two sliding units to be replaced with double casements*

**Right Side:**

*One opening - Slider to be replaced with Double Casement*

**Rear:**

*Three openings – Each sliding unit to be replaced with a double-casement*

**Left Side:**

Four openings –

First Floor @ Rear – Sliding unit to be replaced with gliding window

*First Floor @ middle – Sliding unit to be replaced with double casement*

First Floor @ front – Sliding unit to be replaced with gliding window

Second Floor @ middle – Sliding unit to be replaced with gliding window

**1/20 Email to Brett Mahaffey:**

Requested dimensions on existing sash and proposed, as well as the dimensions for the existing and proposed slider vertical meeting rail and mullion for double casements.