The building was originally submitted to HDC with the second and third level exterior material consisting of a James Hardie Reveal Panel with Recessed Trim. This created a horizontal and vertical grid pattern The window heads and sills provided the horizontal element while the window edges provided the vertical element. This exterior system, however, is not being manufactured by James Hardie until further notice. They are only able to produce their more popular, basic lap siding products currently.

We have selected a new material for HDC review and consideration. The product Western Reveal 1.0 by Western States Metal Roofing. The metal siding will be orientated vertically with a an 18” face and 1” reveal. The attachment type is concealed fastening. The color selected, Colonial Red, matches very closely the original submittal. Drawings, product cut sheets and revised renderings have been provided as requested.