Window Renovation – North and West Elevations (6 photos):

25, 26, 29, 38, 40, 41 – Original windows still installed, will be removed and renovated.

All remaining vinyl windows on these elevations will be left as is (see note below). All break metal trim will be removed and the trim underneath will be repaired and painted.

vinyl

\*\*NOTE\*\* Only original windows are being used. These are all wood construction, some double hung and some fixed, and some operable as indicated. If approved where original windows are not found, I would like to custom construct the window with the configuration it was originally made to using hardwoods and period hardware to match the rest of the house.